   #[1]iso2mesh: a Matlab/Octave-based mesh generator

Frequently asked questions about iso2mesh

          1. [2]I am getting a "Two subfaces ... are found intersecting
          each other" error, what should I do?

          2. [3]After mesh generation, the surface plot looks messed up,
          what was wrong?

          3. [4]Matlab complains about imread, imclose or imfill missing

          4. [5]iso2mesh failed when writing files to disk

          5. [6]When displaying a surface produced by iso2mesh, there are
          many holes, how to fix this?

          6. [7]Subroutine meshresample returns an empty mesh, why?

          7. [8]Which meshing option should I choose?

          8. [9]How do I control mesh density in iso2mesh?

          9. [10]How to mesh a domain containing multiple isolated objects
          ?

1. I am getting a "Two subfaces ... are found intersecting each other" error, what should I do?

   This is the most frequently encountered problem using this toolbox.
   There are three possible causes of this error:

1. the volume you are trying to mesh contains joint regions between more than 2 materials

   This is most likely happening when you see the above error message. Try
   to plot your volume slice by slice, and pay attention to any voxels
   whose neighbors have more than 2 different values. If this is the case,
   you can only use this type of input with vol2mesh/v2m with 'cgalmesh'
   option as the "method" parameter. If you use either "simplify" or
   "cgalsurf" (default) options, iso2mesh will fail. If for some reason
   you have to use these options, here are two possible temporary
   work-arounds:
    1. if there are not many junction voxels, you may want to manually
       edit your image and disconnect the regions that share the same
       boundary and make sure all the sub-regions are either completely
       disjointed, or completely enclosed by another.
    2. merge the regions that have shared boundaries, and mesh the
       resulting merged volume; after you get the tetrahedra, compute the
       centroid of each element in the merged domain (identified by their
       labels), and map them back to your original segmented image;
       determine the original region id using the voxel containing the
       centroids.

   If you have any better suggestions to enable iso2mesh to handle this
   situation, please let [11]me know.

2. you are using 'simplify' method to mesh a complex domain

   There are two possible methods for volume-to-surface conversion,
   'simplify' and 'cgalsurf'. The second method always returns a
   well-posed surface where no self-intersecting elements present;
   however, the 'simplify' approach does not. The default method for
   vol2mesh/vol2surf (v2m/v2s) is 'cgalsurf'. If you have to use
   'simplify', you may have to experiment different surface densities for
   the surface extraction. You may lucky enough to find a working
   configuration, but very likely, you may not. Please use 'cgalsurf'
   option whenever possible.

3. your surface mesh is too coarse and intersects the enclosed surfaces

   The mesh extraction will represent the region boundaries by a sheet of
   triangles. Near sharp edges, this representation may generate a rounded
   edge and does not exactly preserve the shape of the original domain. If
   you happen to mesh a thin layer of material, the resulting surface may
   intersect each other at sharp edges if your surface element is too big.
   Please use a small opt.radbound value to run the mesh generation again.

2. After mesh generation, the surface plot looks messed up, what was wrong?

   It is very likely you incorrectly used the output variables. The output
   of vol2mesh or surf2mesh include elem: the tetrahedral element indices,
   and face: the surface triangle indices. But be careful, both of these
   two arrays have an additional column. The last column is a label field,
   indicating the origin (sub-region) of the elements. You should never
   use the last columns of these two arrays for plotting. To make a
   correct surface plot, you should use something like
 trisurf(face(:,1:3),node(:,1),node(:,2),node(:,3));

   and don't use the full face array as the first parameter.

   If you are using iso2mesh newer than 0.9.8, you can use a function
   called "plotmesh" to visualize the produced surfaces and volumes. The
   script will attempt to recognize the extra column of "face" by using
   the Euler characteristics and automatically ignore it if present.

3. Matlab complains about imread, imclose or imfill missing

   Under the sample/ directory, demo_vol2mesh_ex2.m requires imread, which
   is a build-in function in matlab, but not in octave. You have to
   install octave-image via apt-get or yum first. In example
   demo_vol2mesh_ex3.m, functions imclose and imfill are needed. These two
   functions can only be found in matlab's image processing toolbox. If
   you don't have this toolbox installed (of course, it is not free), you
   can simply pass this example. For octave, unfortunately, these
   functions do not exist yet, and hopefully someone can fill them in
   soon.

4. iso2mesh failed when writing files to disk

   If you are working on a multi-user workstation, and multiple users were
   using iso2mesh, some temporary files may have a conflict in read/write
   permission under /tmp directory. If user A runs iso2mesh first, and
   user B will get this error, because iso2mesh fails to create the
   temporary files as it does not have the permissions to overwrite those
   files created by A. To solve this issue, please define your own
   temporary folder, or set your session id, you can find more info at
   [12]Advanced page.

5. When displaying a surface produced by iso2mesh, there are many holes, howto fix this?

   The node orders in the output surface mesh are random, some are
   oriented clockwise, some are counter-clockwise. This will make OpenGL,
   or OpenGL based applications, render the surface with different
   materials. To correct this, you can simply call
 [newnode,newface]=meshcheckrepair(node,face);

   and the new surface: [newnode,newface] will have consistent
   orientations. Again, be careful if you are using the face output from
   vol2surf/v2s, it has an extra column. You only need to use the first 3
   columns in the face array when making plots.

6. Subroutine meshresample returns an empty mesh, why?

   When the input surface mesh contains topological defects, such as
   non-manifold nodes, the meshresample() subroutine will not proceed and
   return an empty mesh (the output message will show "0 total edges
   collapsed"). In this case, you need to first call meshcheckrepair()
   subroutine to fix your input mesh, and them pass it to meshresample. An
   example is shown below:
  [no2,fc2]=meshcheckrepair(node_in,face_in);
  [node_out,face_out]=meshresample(no2,fc2,0.2);

   (this issue is automatically corrected in iso2mesh 0.8 or newer)

7. Which meshing option should I choose?

   Iso2mesh provides 3 options for v2m and vol2mesh, namely, 'cgalmesh',
   'cgalsurf' and 'simplify'. Some users may get confused which one to
   use. In fact, we were hoping not to put users in this situation, as
   iso2mesh was designed for simplicity and efficiency. Unfortunately, we
   haven't really found a single option that works for all of the
   situations, and each of the 3 options have there good and bad sides.

     * cgalmesh: this is the most powerful option of all, and is
       potentially the ideal candidate as the default option. With
       'cgalmesh', iso2mesh can easily process a binary volume and a
       volume with multi-region labels with good speed and robustness. It
       can produce both volumetric and surfaces meshes at the same time,
       and clearly labels the element and surfaces for each individual
       sub-region. However, it is not perfect. It can not extract
       iso-surfaces from a gray-scale image. When you want to control mesh
       densities near a specific isosurface (such as [13]this case),
       cgalmesh option is not as flexible as the other two. In short,
       cgalmesh is the best choice for producing uniform-sized meshes from
       an arbitrary segmented volume.
     * cgalsurf: cgalsurf option produces surface and volumetric meshes
       with a standard 2-step process as shown in the [14]workflow. When
       extracting multiple isosurfaces, it will do the extraction
       sequentially. The strengths of cgalsurf include 1) all the
       extracted surfaces are guaranteed to be free of self-intersecting
       elements, individually, and 2) it can handle gray-scale volumes.
       The main issue for cgalsurf is when multiple isosurfaces overlap to
       each other, v2m/vol2mesh will break as the combined surface
       contains self-intersecting elements. In short, cgalsurf is the best
       option when multiple sub-regions are disconnected, or one enclosing
       another.
     * simplify: this is as flexible as cgalsurf, but it is not as
       reliable. After the mesh simplification, a surface may become
       self-intersecting and v2m/vol2mesh will stop working. However, when
       you only have a dense surface to start with, this is the only
       option you can use.

   To make it easy to remember:
    1. when meshing a simple binary volume, 'cgalmesh' and 'cgalsurf' are
       both good choices
    2. when meshing a segmented volumes with multiple sub-regions, use
       'cgalmesh'
    3. when meshing a gray-scale volume, use 'cgalsurf'
    4. when other options fail, try 'simplify'.

8. How do I control mesh density in iso2mesh?

   Iso2mesh uses two parameters to quantitatively control the mesh
   density. In v2m or vol2mesh, parameter opt sets the maximum edge length
   of the surface triangles (i.e. controlling the density of the mesh on
   the surface), and maxvol sets the maximum tetrahedron volume.

   If you want to let the mesh be denser on the surface and coarser
   inside, you can use a small opt value and a large maxvol value.

   If you want to control the surface mesh density so that it adapts
   depending on the curvature, you can do so by defining opt as a struct,
   and set the opt.radbound and opt.distbound values. You can find
   examples from [15]this presentation (slide 15). This example can also
   be accessed from iso2mesh/sample/demo_helloworld.m

9. How to mesh a domain containing multiple isolated objects ?

   This is a known issue with the CGAL [16]surface mesher and [17]3D
   mesher. A bug report has been filed [18]here, but it was not known if
   any fix has been applied upstream.

   For v2m/v2s with a 'cgalmesh' option, a simple work-around is to remove
   zero-voxels by adding 1 to the 3D image. Then cgalmesher should be able
   to recover all inclusions, along with the background. You can then
   remove the background by checking the domain ID. For example:

  [no,el]=v2m(uint8(img+1), [], opt, maxvol, 'cgalmesh');
  el=el(find(el(:,5)>1),:);
  [no,newel]=removeisolatednode(no(:,1:3),el(:,1:4));
  newel(:,5)=el(:,5)-1;

   If the target domain is a binary image, there is another work-around:
function [node,elem]=meshisolatedobj(img,opt,maxvol)
%
% Usage:
%    [node,elem]=meshisolatedobj(img,opt,maxvol)
%    Author: Qianqian Fang <fangq at nmr.mgh.harvard.edu>
%
img=logical(img);
[bin,regionnum]=bwlabeln(img,6);
node=[];
elem=[];

for regionid=1:regionnum
    fprintf(1,'meshing region #%d ...\n',regionid);

    [no,el]=v2m(bin==regionid,0.5,opt,maxvol);

    % merge the resulting mesh with other regions
    el(:,5)=regionid;
    el(:,1:4)=el(:,1:4)+size(node,1);
    if(regionid>1)
        elem=[elem;el];
        node=[node;no];
    else
        node=no;
        elem=el;
    end
end

   This function only works in Matlab because function bwlabeln is not
   available in Octave.

References

   1. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?action=rss
   2. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/FAQ#I_am_getting_a_Two_subfaces_are_found_intersecting_each_other_error_what_should_I_do
   3. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/FAQ#After_mesh_generation_the_surface_plot_looks_messed_up_what_was_wrong
   4. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/FAQ#Matlab_complains_about_imread_imclose_or_imfill_missing
   5. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/FAQ#iso2mesh_failed_when_writing_files_to_disk
   6. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/FAQ#When_displaying_a_surface_produced_by_iso2mesh_there_are_many_holes_how_to_fix_this
   7. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/FAQ#Subroutine_meshresample_returns_an_empty_mesh_why
   8. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/FAQ#Which_meshing_option_should_I_choose
   9. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/FAQ#How_do_I_control_mesh_density_in_iso2mesh
  10. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/FAQ#How_to_mesh_a_domain_containing_multiple_isolated_objects
  11. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?FangQ
  12. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Advanced
  13. http://iso2mesh.sourceforge.net/upload/head_mesh.jpg
  14. http://iso2mesh.sourceforge.net/cgi-bin/index.cgi?Doc/Workflow
  15. http://iso2mesh.sf.net/upload/iso2mesh_a_one_liner_mesh_generator.pdf
  16. http://www.cgal.org/Manual/latest/doc_html/cgal_manual/Surface_mesher/Chapter_main.html
  17. http://www.cgal.org/Manual/latest/doc_html/cgal_manual/Mesh_3/Chapter_main.html
  18. http://cgal-discuss.949826.n4.nabble.com/missing-objects-when-meshing-a-3D-image-with-multiple-disconnected-inclusions-td3349283.html
